SECURITY SYSTEM DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1___28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2___28 23 00 VIDEO SURVEILLANCE
LEVEL 3___28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS
1.0	Purpose
A.	This document describes the specification of the Ax47R2, Ax47R4, Ax67R2, and Ax67R4 outdoor network dome cameras.
2.0 Specifications
2.1	Manufacturer
A.	i3 International Inc., Scarborough, Ontario, Canada M1K 5H4,
Telephone: 416.261.2266.
B.	The manufacturer shall warrant the camera to be free from defects in material and workmanship for three years from the purchase date. 
C.	All systems and components shall have been thoroughly tested, proven in actual use, and have i3 Superior five-year warranty.
D.	Technician with a current and valid i3 Dealer Certification shall be on site at all times during installation.

2.2 General Camera Specifications
A.	This product shall be manufactured by a firm whose quality system is in compliance with the ISO 9001:2008.
B.	All materials furnished under this item shall be compliant with 802.3 Ethernet standards. 
C.	These network cameras shall be fully compatible with i3 International SRX-Pro series.  
D.	The two models Ax47R2 and Ax47R4 shall be 1.3 megapixel cameras.
E.	The two models Ax67R2 and Ax67R4 shall be 3 megapixel cameras.
F.	The 4 models shall use an Auto Iris control.
G.	The Ax47R2 and Ax67R2 shall use a 2.8mm, F1.8 lens.
H.	The Ax47R4 and Ax67R4 shall use a 4mm F1.6 lens.
I.	The Ax47R2 shall have an angle of view of 93° (H) ~ 70° (V).
J.	The Ax47R4 shall have an angle of view of 63° (H) ~ 47° (V).
K.	The Ax67R2 shall have an angle of view of 100°(H) ~ 74° (V).
L.	The Ax67R4 shall have an angle of view of 68° (H) ~ 51° (V).
M.	These network cameras shall meet or exceed the following design and performance specifications.

2.3 Electric Specifications
A.	The network cameras shall provide mechanical (ICR) low-light capabilities with minimum illumination of 0.3 Lux (Color mode) AGC=36dB 50 IRE, 0.1 Lux (BW mode) AGC=36dB 50 IRE, and 0 Lux with Infrared ON.
B.	The network cameras shall have an Infrared distance of 25m (approx. 82’).
C.	The network cameras shall offer triple streaming and video compression of H.264 and Motion JPEG.
D.	The network cameras shall use 3D digital noise reduction technology.
E.	The network cameras shall use digital wide dynamic range (WDR).
F.	The network cameras shall use an electric shutter NTSC: 1/7.5~1/10000 sec or PAL: 1/6.25 ~ 1/10000 sec.
G.	The network cameras shall use back light compensation configurable to six selectable areas when turned ON.
H.	The network cameras shall provide for on-board (Edge) storage with one microSD/SDHC/SDXC slot up to 64GB. Card sold separately.
I.	The network cameras shall provide the following special features: Privacy Mask, Mirror Flip, Corridor View, Edge Defocus Detection, Smart IR, FTP Recording, and Digital Defog

2.4 Network Specifications
A.	The Ax47R2 and the Ax47R4 shall offer 1.3MP (1280x960) resolution at frame rates of 30fps/25fps.
B.	The Ax67R2 and the Ax67R4 shall offer 3MP (2048x1536) resolution at frame rates of 30fps/25fps.
C.	The network cameras shall use the following network protocols: IPv4, TCP/IP, UDP/IP, FTP, ICMP, ARP, DHCP, HTTP, SMTP, IGMP, RTSP, RTP, RTCP, and SNMP.
D.	The network cameras shall have security access in the form of multiple privilege control with password and allow one administrator and five operators/users.

2.5 Mechanical Specifications
A.	The network cameras shall allow Pan: >360°, Tilt: 20°-90°, and Rotation: ±175° angle adjustments.
B.	The network cameras shall have Ø112mm x 82mm (Ø4.4" x 3¼") dimensions.
C.	The network cameras shall weigh 460g (approx.1 lbs.).
D.	The network cameras shall have one RJ45 network connector.

2.6 Power Supply
A.	The network cameras shall require IEEE 802.3af, class 3 power supply.
B.	The network cameras shall consume a maximum of PoE 8.5W.

2.7 Environment
A.	The operating temperature of the network cameras shall be between -40°C and 50°C (-40°F - 122°F).
B.	The operating humidity of the network cameras shall not exceed 90% non-condensing.
C.	The network cameras shall be able to power on at temperatures -20°C (-4°F) and above.
D.	The network cameras shall power back on after a power outage only if the ambient temperature did not drop below -20°C (-4°F).

2.8 Regulations
A.	The network cameras shall adhere to FCC Class B, CE, RoHS, UL, IP67, IK10, ONVIF regulations.